|  |  |  |  |
| --- | --- | --- | --- |
| **Jurisdiction** | **Submitted by** | **Unmetered Device** | **Load as tested (W)** |
| ALL | HBW Lighting | AEC 0F2 4.7-4M | 68.9W |
| ALL | HBW Lighting | AEC 0F2 4.7-5M | 84.7W |
| ALL | HBW Lighting | AEC 0F2 4.7-8M | 137W |
| ALL | HBW Lighting | AEC 0F2H1 HPO27 4.7-8M | 140.9W |